Last poring part from burrete to erlnemeyer flask
In acid-base titration when we transfer 0.1M NaoH from burette to Erlenmeyer flask in last poring part ,we use precise mode or realistic mode.
ChemCollective-Virtual-Labs Acid-base-Titrations 01-02 min 0-10 sec 01-07-21, 3:25 p.m. sanjitpalai03@gmail.com

#### Answers:

hi.
To transfer the last portion accurately it is good to use precise transfer mode. Using precise transfer method we can transfer upto three decimals places. So end result will be accurate.
01-07-21, 4:38 p.m. madhurig

Click here to reply/comment online